*Please complete form and send by mail to:* [*service@boule.se*](mailto:service@boule.se) *or submit at* [*https://boule.com/service-reports/*](https://boule.com/service-reports/)

**Boule Diagnostics AB** **Instrument installed by:**  
Att. Service Name of distributor: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ **Domnarvsgatan 4** Name (block letters): \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ **SE-163 53 Spånga; Sweden** Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

# Installation of instrument

**Instrument**:  
 Medonic M-series/ M32  Serial number: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Reagents**:  
Diluent: Lot number: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Exp. Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  
  
Lyse: Lot number: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Exp. Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

|  |  |  |
| --- | --- | --- |
| 1. Unpacking | **OK** | **Comments:** |
| Sealing of packing box intact |  |  |
| No damage to packaging |  |  |
| Correct accessories |  |  |
| Within EU: Manual in local language distributed to customer |  |  |
|  |  |  |
| 1. Bringing to operation | **OK** | **Comments:** |
| Connecting tubing for hemolysing reagent, diluent and waste |  |  |
| No screen with indication number when the instrument is switched on |  | No of indication(s): |
| Filling system |  |  |
| Control of background count, values within range |  |  |
| Analyse a control, and make sure that the values are within reference ranges |  |  |

Other comments: