*Please complete form and send by mail to:* *service@boule.se* *or submit at* [*https://boule.com/service-reports/*](https://boule.com/service-reports/)

**Boule Diagnostics AB** **Instrument installed by:**
Att. Service Name of distributor: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ **Domnarvsgatan 4** Name (block letters): \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ **SE-163 53 Spånga; Sweden** Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

# Installation of instrument

**Instrument**:
 Medonic M-series/ M32 [ ]  Serial number: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Reagents**:
Diluent: Lot number: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Exp. Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Lyse: Lot number: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Exp. Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

|  |  |  |
| --- | --- | --- |
| 1. Unpacking
 | **OK** | **Comments:** |
| Sealing of packing box intact | [ ]  |  |
| No damage to packaging | [ ]  |       |
| Correct accessories | [ ]  |       |
| Within EU: Manual in local language distributed to customer | [ ]  |       |
|  |  |  |
| 1. Bringing to operation
 | **OK** | **Comments:** |
| Connecting tubing for hemolysing reagent, diluent and waste | [ ]  |  |
| No screen with indication number when the instrument is switched on | [ ]  | No of indication(s):  |
| Filling system | [ ]  |  |
| Control of background count, values within range | [ ]  |  |
| Analyse a control, and make sure that the values are within reference ranges | [ ]  |  |

Other comments: